Aqua Tank Type III Instructions 2016

Basic Parts List –

1. Liner
2. 1” schedule 40 top & bottom rail pieces
3. Upright posts and outboard supports
4. Storage bag

Instructions –

1. Remove and inspect all parts being sure you have everything you need
2. Unfold liner and spread the floor out removing all wrinkles in the floor. The liner side walls will lay inward.
3. Take the top & bottom rail pieces and place them along the outside of the liner and place the upright posts in the corners. All upright posts have 1” aluminum tubing with spring snaps installed; these are to accept the top & bottom rail pieces which have countersunk holes drilled to accept the spring snaps.
4. There is a pocket located at the top of the liner side wall with cutouts for the top rail pieces, slide the top rail piece into the liner pocket until both ends are exposed at the cutouts. There is no pocket for the bottom rail, it is not needed.
5. Insert the top rail piece into the upright piece until it “snaps” into the hole then the bottom rail into the bottom of the upright.
6. The opposite end of the top rail piece should be exposed and ready to install the next upright piece. Snap the 2nd upright piece into the top and bottom rails.
7. Insert another top rail piece into the liner then the upright post. Continue this until you have returned to the first corner post you started with.
8. Slide the last top & bottom rail piece into the corner piece