

7202 SE International Ct.

P.O. Box 3404

Bartlesville, OK. 74006

918-333-2000

800-260-9950

918-333-2004 Fax

E-Mail: sales@huskyportable.com

[www.huskyportable.com](http://www.huskyportable.com)

 “Leader of the Pack”

Quick Dump Lacing Instructions –

You will use the standard Lacing Instructions for three sides of the tank. When you come to the Quick Dump side follow instructions below.

Prep Your Frame –

1. Using a 3/16” drill (or something similar) drill out the center of the existing rivets which are located on the Quick Dump door.
2. Remove old liner
3. Place new liner in the frame according to where the Quick Dump is located.
4. Start lacing the liner on the opposite side of the Quick Dump in the center of the frame. Leave enough rope on both sides of the starting point so they will meet on the opposite side of the frame.
5. When you reach one side of the Quick Dump door tie the rope off here.
6. Continue lacing the opposite side until you reach the other side of the Quick Dump door and tie off there as well. DO NOT tie off directly on the door.
7. Once you have tied both sides off the last step is two line up the preexisting holes on the Quick Dump door to the liner hem. There will not be holes in the liner. Mark the frame holes on the liner and take a leather punch or scratch awl (or something similar) to create the holes to accept the rivets.
8. Rivet the liner to the Quick Dump door, hook the liner to the original hooks and you are ready to fill your tank.

Any questions call Husky Portable Containment, 800-260-9950